# Manhole cover SD11, for flush fitting, lightweight design

**Manhole cover,** lift-off design, for flush fitting, weather- proof, rectangular type, load-bearing up to 500 kg/m²,   
made of 1.4307 (AISI 304 L) stainless steel.

**The cover** consists of a stainless steel tear pattern plate, with additional bracing on the bottom according to static requirements, certified slip resistance – grip coefficient USRV 54, with a low-wear seal on the cover bottom side,   
lockable with hexagon screws.

**Frame** made from U-profile, provided for installation in an existing rabbet.

Manhole cover and frame shielded arc-welded, acid- treated in a pickling bath and passivated.

Operating key included.

**Options:**

➤ 1.4404 (AISI 316 L) stainless steel

➤ With hinges, stainless steel gas-assisted spring dampers and integrated arrestor which can only be undone by hand

➤ For installation into a manhole neck

➤ Fixing material and foam rubber gasket

➤ Magnetic contact (cover open/shut indicator)

➤ Safety guard / barrier

➤ Safety guard / antifall guard

➤ Multi-part cover