# Sliding hatch cover SD12

**Sliding hatch cover,** completely made of 1.4307 (AISI 304 L) stainless steel, with smooth finish.

**The cover** is made of a stable stainless steel plate and equipped with plastic rollers and maintenance-free   
journal bearings. The cover is installed in an external guide rail and cannot be removed. Locking when closed   
is possible by a cylindrical lock.

**The rails** consist of 60/40/2 mm rectangular section fixed with dowels along the rail edge.

Manhole cover and rails shielded arc-welded, acid-treated in a pickling bath and passivated.

Operating key included.

Dimensions according to individual requirements Available options:

1. straight version
2. circular version

The sliding cover provides access to downward leading stairs.

**Options:**

➤ 1.4404 (AISI 316 L) stainless steel

➤ Special design available on request