# Entrance handle SiS 5 HB

**Entrance handle,** completely made of 1.4307 (AISI 304 L) stainless steel.

Consisting of bent pipe 33.7 x 2.0 mm with fixing plates for wall fixing.

Entrance handle, completely shielded arc welded, acidtreated in a pickling bath and passivated.

**Options:**

➤ 1.4404 (AISI 316 L) stainless steel

➤ Stainless steel fixing material: stud anchors